!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!IMPORTANT!!!!!!!!!!!!!!!!!!!!!!!!!!!!

This dataset comes from the Turing Institute, Glasgow, Scotland.

If you use this dataset in any publication you must acknowledge this

source.

!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!!

NAME

vehicle silhouettes

PURPOSE

to classify a given silhouette as one of four types of vehicle,

using a set of features extracted from the silhouette. The

vehicle may be viewed from one of many different angles.

PROBLEM TYPE

classification

SOURCE

Drs.Pete Mowforth and Barry Shepherd

Turing Institute

George House

36 North Hanover St.

Glasgow

G1 2AD

CONTACT

Alistair Sutherland

Statistics Dept.

Strathclyde University

Livingstone Tower

26 Richmond St.

GLASGOW G1 1XH

Great Britain

Tel: 041 552 4400 x3033

Fax: 041 552 4711

e-mail: alistair@uk.ac.strathclyde.stams

HISTORY

This data was originally gathered at the TI in 1986-87 by

JP Siebert. It was partially financed by Barr and Stroud Ltd.

The original purpose was to find a method of distinguishing

3D objects within a 2D image by application of an ensemble of

shape feature extractors to the 2D silhouettes of the objects.

Measures of shape features extracted from example silhouettes

of objects to be discriminated were used to generate a class-

ification rule tree by means of computer induction.

This object recognition strategy was successfully used to

discriminate between silhouettes of model cars, vans and buses

viewed from constrained elevation but all angles of rotation.

The rule tree classification performance compared favourably

to MDC (Minimum Distance Classifier) and k-NN (k-Nearest Neigh-

bour) statistical classifiers in terms of both error rate and

computational efficiency. An investigation of these rule trees

generated by example indicated that the tree structure was

heavily influenced by the orientation of the objects, and grouped

similar object views into single decisions.

DESCRIPTION

The features were extracted from the silhouettes by the HIPS

(Hierarchical Image Processing System) extension BINATTS, which

extracts a combination of scale independent features utilising

both classical moments based measures such as scaled variance,

skewness and kurtosis about the major/minor axes and heuristic

measures such as hollows, circularity, rectangularity and

compactness.

Four "Corgie" model vehicles were used for the experiment:

a double decker bus, Cheverolet van, Saab 9000 and an Opel Manta 400.

This particular combination of vehicles was chosen with the

expectation that the bus, van and either one of the cars would

be readily distinguishable, but it would be more difficult to

distinguish between the cars.

The images were acquired by a camera looking downwards at the

model vehicle from a fixed angle of elevation (34.2 degrees

to the horizontal). The vehicles were placed on a diffuse

backlit surface (lightbox). The vehicles were painted matte black

to minimise highlights. The images were captured using a CRS4000

framestore connected to a vax 750. All images were captured with

a spatial resolution of 128x128 pixels quantised to 64 greylevels.

These images were thresholded to produce binary vehicle silhouettes,

negated (to comply with the processing requirements of BINATTS) and

thereafter subjected to shrink-expand-expand-shrink HIPS modules to

remove "salt and pepper" image noise.

The vehicles were rotated and their angle of orientation was measured

using a radial graticule beneath the vehicle. 0 and 180 degrees

corresponded to "head on" and "rear" views respectively while 90 and

270 corresponded to profiles in opposite directions. Two sets of

60 images, each set covering a full 360 degree rotation, were captured

for each vehicle. The vehicle was rotated by a fixed angle between

images. These datasets are known as e2 and e3 respectively.

A further two sets of images, e4 and e5, were captured with the camera

at elevations of 37.5 degs and 30.8 degs respectively. These sets

also contain 60 images per vehicle apart from e4.van which contains

only 46 owing to the difficulty of containing the van in the image

at some orientations.

ATTRIBUTES

COMPACTNESS (average perim)\*\*2/area

CIRCULARITY (average radius)\*\*2/area

DISTANCE CIRCULARITY area/(av.distance from border)\*\*2

RADIUS RATIO (max.rad-min.rad)/av.radius

PR.AXIS ASPECT RATIO (minor axis)/(major axis)

MAX.LENGTH ASPECT RATIO (length perp. max length)/(max length)

SCATTER RATIO (inertia about minor axis)/(inertia about major axis)

ELONGATEDNESS area/(shrink width)\*\*2

PR.AXIS RECTANGULARITY area/(pr.axis length\*pr.axis width)

MAX.LENGTH RECTANGULARITY area/(max.length\*length perp. to this)

SCALED VARIANCE (2nd order moment about minor axis)/area

ALONG MAJOR AXIS

SCALED VARIANCE (2nd order moment about major axis)/area

ALONG MINOR AXIS

SCALED RADIUS OF GYRATION (mavar+mivar)/area

SKEWNESS ABOUT (3rd order moment about major axis)/sigma\_min\*\*3

MAJOR AXIS

SKEWNESS ABOUT (3rd order moment about minor axis)/sigma\_maj\*\*3

MINOR AXIS

KURTOSIS ABOUT (4th order moment about major axis)/sigma\_min\*\*4

MINOR AXIS

KURTOSIS ABOUT (4th order moment about minor axis)/sigma\_maj\*\*4

MAJOR AXIS

HOLLOWS RATIO (area of hollows)/(area of bounding polygon)

Where sigma\_maj\*\*2 is the variance along the major axis and

sigma\_min\*\*2 is the variance along the minor axis, and

area of hollows= area of bounding poly-area of object

The area of the bounding polygon is found as a side result of

the computation to find the maximum length. Each individual

length computation yields a pair of calipers to the object

orientated at every 5 degrees. The object is propagated into

an image containing the union of these calipers to obtain an

image of the bounding polygon.

NUMBER OF CLASSES

4 OPEL, SAAB, BUS, VAN

NUMBER OF EXAMPLES

Total no. = 946

No. in each class

opel 240

saab 240

bus 240

van 226

100 examples are being kept by Strathclyde for validation.

So StatLog partners will receive 846 examples.

NUMBER OF ATTRIBUTES

No. of atts. = 18

BIBLIOGRAPHY

Turing Institute Research Memorandum TIRM-87-018 "Vehicle

Recognition Using Rule Based Methods" by Siebert,JP (March 1987)